**All PPE requirements apply to all personnel working in these areas and to ensure compliance with the OSHA standard for Personal Protective Equipment 29 CFR 1910.132, for the general rules for PPE see document # 1390.**

**Melting and Casting**

Melting and Casting PPE is in document # 1007.

**Rolling and Finishing**

|  |  |
| --- | --- |
| **Operation / Location** | **PPE Required** |
| **Rolling & Finishing & Heat Treat** | * **Hard Hat** * **Metatarsal Boots** * **Safety Glasses** * **Hearing Protection** * **Long Sleeves and Pants** |
| **Roll Shop** | * **Hard Hat** * **Metatarsal Boots** * **Safety Glasses** * **Hearing Protection** |
| **Cutting or Burning** | * **Hard Hat** * **Metatarsal Boots** * **Safety Glasses** * **Hearing Protection** * **Green Jacket** **or Flame-Retardant Shirt** * **Leather Gloves** * **Faceshield** |
| **Shipping** | * **Hard Hat** * **Metatarsal Boots** * **Safety Glasses** * **Hearing Protection** * **Long Sleeves and Pants** |